HOLLY STREET HOMEOWNERS’ ASSOCIATION
ARCHITECTURAL CONTROL SUBMITTAL

(Plans can be submitted Monday through Friday 8:30 a.m. to 5:30 p.m. to Holly Street Homeowners Association, 2400 So. 57th St., Temple, Texas 76504)
Date Received: ____________________________

Legal Description:  _________________________  Owner:  ____________________________

Street Address:  ____________________________
Address: ___________________________

Square Footage (total conditioned area):


  ___________________________



_____________________________
Phone: ____________________________

Architect/Designer: ________________________
Builder: ___________________________

Address: _________________________________
Address: __________________________

Phone:  __________________________________
               __________________________








Phone: ______________________(Work)









______________________(Mobile)









______________________(Fax)

Applicant Signature: ___________________________________________________________





**********************************

Plan Submittal Checklist

A complete application package contains the following:

I. Site Plan (Two Copies)—site plan at 1”=10’ minimum:

_____  
All property lines, easements, building lines (including decks, patios, all improvements), North arrow

_____
Topo required showing existing contours

_____
Setbacks

_____
Easements and encroachments

_____
Dimensions from proposed structure to property lines

_____
Utility locations and proposed trench lines

_____
Drainage plan

_____
Proposed drives, walks, and any other flatwork or improvements

_____
HVAC units location and appropriate screening

_____
Location of utility boxes and meters

_____
Written description of post development drainage patterns or grading plan

_____
Silt fencing location

_____
Dumpster location

_____
Port-a-let location

II. Architectural Plans (Two Copies)—(All plans for custom sections must be site specific—No “Mass Production” drawings accepted):

_____
¼” scale—driveway, sidewalks, patios, covered porches, decks, tree survey

_____
Square footage calculations of conditioned area on each level

_____
Minimum four elevations (front, rear, left, right) with grade shown

_____
Clearly marked exterior materials

_____
Exterior must be 75% masonry designated by architect plans.  

_____
Fencing (design and color included)

_____
Roof pitches indicated

_____
Building height measured per appropriate deed restrictions

III. Material Samples—Sample Board/File (All samples must be attached securely inside of a manila folder):

_____
Exterior paint—color samples (chips)—no larger than 4”x4”

_____
All exterior colors of trim, accents, and stucco walls must be designated on all plans and elevations.  Sample paint chips must be no larger than 4”x4”.

_____
Brick or stone—small sample or small samples if multi-color—no larger than 4”x4” or photograph with description (Acme brick style #)

_____
Roofing material and color, including documentation of weight and warranty—copy of brochure not entire sample panel—small sample 4”x4”. Photograph is acceptable.

IV. Landscape Plans (Two Copies):

_____
Size, type and location of all landscaping plants or materials—engineering plans will be required as necessary.

_____
Location, materials and elevations of any proposed retaining walls

_____
Location and materials of any proposed fencing

All other site improvements such as pool, fountains; spas; fences; playscapes; etc. not on original plans with complete details must be submitted for approval.  

      A complete application package contains the following documents:

      Site/Construction Plan (1” = 10’ minimum)

Floor Plans (1/4” = 1’0”)

Roof Plan (1/4” = 1’0”)

Exterior Elevations and Details (1/4’ = 1’0” minimum)

Sample Board with Exterior Colors

The Architectural Control Committee will approve or disapprove all plans and requests within thirty (30) days after submission. In the event the Architectural Control Committee fails to take any action within thirty (30) days after requests have been submitted, approval will be presumed, and this procedure will be deemed to have been fully complied with. 

